**L20 DOORS/SHUTTERS/HATCHES**   
490 AUTOMATIC DOORS:

Manufacturer:

ASSA ABLOY Entrance Systems Limited, Unit 9 Windmill Business Village, Sunbury-on-Thames, Middlesex, TW16 7DY. Tel: 0333 006 3443. Email: [architect.uk.entrance@assaabloy.com](mailto:architect.uk.entrance@assaabloy.com) Web: [www.assaabloyentrance.co.uk](http://www.assaabloyentrance.co.uk)

Models:  
ASSA ABLOY SL530 C Curved / Semi-Circular / 360 deg Circular Sliding Door System, complete with ASSA ABLOY SL530 operator providing automated operation of the sliding door leaves. Verified with 3rd party EPD documentation. System including normal installation to comply with BS7036-0/EN16005.

Door System:

ASSA ABLOY SL530 C Curved / Semi-Circular / 360 deg Circular sliding door:

* Profiles: ASSA ABLOY curved profile system
* Doors mounted: Inside of curve / Outside of curve
* Glass type: 8mm laminated in curved walls and door leaves
* Direction: Bi-parting
* Sidelights: YES / NO
* Dust protection roof: YES / NO
* Water resisting roof: YES / NO
* Extended Canopy: YES / NO
* Spotlights: YES / NO
* Rubber Matting inside door: YES / NO
* Finish: Anodized / RAL powder coat finish: Ref.

Activation and control system:

ASSA ABLOY Combined uni-directional and threshold presence detection entry/exit activator.   
Morning entry switch: YES / NO

Standard equipment:

Monitored emergency opening and threshold presence detection safety system.

Intelligent traffic flow control optimizing opening widths and hold open times

Sidelight Safety: MONITORED PRESENCE DETECTION   
Operation Mode Selector: Digital ASSA ABLOY 6 position / Keyed ASSA ABLOY 6 position

Electric Locking Required: FAIL SAFE / FAIL SECURE / BI-STABLE / NONE

Integrated Air Curtain: YES / NO

Mechanical Locking mechanism:

Mechanical Hook lock: ONE / TWO, positioned in meeting door stiles.

Euro Cylinder: Key with thumb turn / Key both sides

Warranty:

Standard 1 YEAR warranty

Extended warranty with two service visits per annum for optimum performance and longevity: 2 YEAR / 3 YEAR / 4 YEAR / 5 YEAR / 10 YEAR

Please consult ASSA ABLOY Entrance Systems Limited technical literature for further details and the quotation for project specific notes.