**L20 DOORS/SHUTTERS/HATCHES**   
490 AUTOMATIC DOORS:

Manufacturer:

ASSA ABLOY Entrance Systems Limited, Unit 9 Windmill Business Village, Sunbury-on-Thames, Middlesex, TW16 7DY. Tel: 0333 006 3443. Email: [architect.uk.entrance@assaabloy.com](mailto:architect.uk.entrance@assaabloy.com) Web: [www.assaabloyentrance.co.uk](http://www.assaabloyentrance.co.uk)

Models:  
ASSA ABLOY SL540 H Hermetic Sliding Door System, complete with ASSA ABLOY SL540 operator providing automated operation of the sliding door leaves. Verified with 3rd party EPD documentation. System including normal installation to comply with BS7036-0/EN16005.

Door System:

ASSA ABLOY SL540 H hermetic sliding door system:

* Profiles: ASSA ABLOY hermetic profile system
* Direction: Single
* Window: Round / Square / none
* Lead lined: YES / NO
* Reveal Plates: YES / NO
* Operator Finish: Anodized / RAL powder coat finish: Ref.
* Door Finish: Formica

Activation and control system:

ASSA ABLOY Push Pad entry/exit activator.

Standard equipment:

Monitored emergency opening and threshold presence detection safety system.

Intelligent traffic flow control optimizing opening widths and hold open times

Sidelight Safety: MONITORED PRESENCE DETECTION / None as trained traffic  
Operation Mode Selector: Digital ASSA ABLOY 6 position / Keyed ASSA ABLOY 6 position

Electric Locking Required: FAIL SAFE / FAIL SECURE / BI-STABLE / NONE

Manual opening mechanism:

Door Handles: ONE / TWO

Warranty:

Standard 1 YEAR warranty

Extended warranty with two service visits per annum for optimum performance and longevity: 2 YEAR / 3 YEAR / 4 YEAR / 5 YEAR / 10 YEAR

Please consult ASSA ABLOY Entrance Systems Limited technical literature for further details and the quotation for project specific notes.